
The ALU-generator (alugen.c) generates the binary look-up-tables
for the ALU. The binary files must be burned into the EPROMs:

Files:
  alu1data.bin     (raw binary image for IC59)
  alu1data-64.bin  (EPROM binary image for 27C64  / IC59)
  alu1data-256.bin (EPROM binary image for 27C256 / IC59)
  alu2data.bin     (EPROM binary image for 27C801 / IC58)   
  aluflags.bin     (EPROM binary image for 27C801 / IC57)

Note: IC59 can be a 27C64 or a 27C256.


Contact:
  Dennis Kuschel
  Kurt-Georg-Kiesinger-Allee 14
  28279 Bremen
  Germany

  email: dennis_k@freenet.de
  web:   http://www.mycpu.eu
